Will Townsend

Dr. E.A. Lu

COSC 370-750

7 April 2021

***Lab 5***

Lab Report: This lab was pretty straightforward. I was able to see the TCP in action which was cool. Wireshark is almost second nature at this point. I completed this lab 100% independently with no help from outside resources (excluding provided content).

1) IP (client): 192.168.1.102 & TCP port # (client): 1161

2) IP (gaia.cs.umass.edu): 128.119.245.12 & TCP port # (gaia.cs.umass.edu): 80

3) IP (Personal): 192.168.95.64 & TCP port # (Personal): 55241

4) The sequence number is 0 and the SYN can be indicated by setting the syn flag to 1

5) The sequence number is also 0. The value is 1 in the acknowledgement field. The client told the destination what value. The values/flags of syn and ack are both 1.

6) Sequence Number of TCP (segment with HTTP POST): 1

7&8) EstimatedRTT: 189.875 ms (when alpha = .125)

|  |  |  |
| --- | --- | --- |
| Sequence # | RTT (ms) | Length |
| 1 | about 190 | 565 |
| 566 | about 189 | 1460 |
| 2026 | about 189 | 1460 |
| 3486 | about 189 | 1460 |
| 4946 | about 190 | 1460 |
| 6406 | about 190 | 1460 |

9) The minimum amount of available buffer space: 5840 bytes. The lack of receiver buffer space doesn’t ever throttle the sender.

10) There are no retransmitted segments. I looked for any repeating segment numbers.

11) The receiver acknowledges 1460 bytes of data in ack. They would double if it was acknowledging every other segment.

12) File size: 177851 bytes / Total time: 7.593 = Throughput: 23,423.021 Bps

13) slowstart phase: Packet 1-13. The data doesn’t take the normal exponential to linear approach as with situation studied prior.

14) My personal shows slowstart phase: Packet 1-219 (this after analysis may be an error on my part)